Exalo Drilling S.A. requirements:

|  |
| --- |
|  |

We undersigned declare that we get acquaint with Exalo Drilling S.A. requirements and our offer is fully compatible with them.

**Bidders Name: …………………………………………………………………….………………………………………………………**

1. **Mongoose Screens**

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Manufacturer Part Number | Requirements | Qty. (15 wells) estimated usage per year |
| 1 | …………………….. | API 35 - mesh 38 | 40 |
| 2 | …………………….. | API 50 - mesh 50 | 30 |
| 3 | …………………….. | API 60 - mesh 70 | 40 |
| 4 | …………………….. | API 70 - mesh 84 | 30 |
| 5 | …………………….. | API 80 - mesh 105 | 90 |
| 6 | …………………….. | API 100 - mesh 120 | 90 |
| 7 | …………………….. | API 120 - mesh 165 | 60 |
| 8 | …………………….. | API 140 - mesh 200 | 30 |
| 9 | …………………….. | API 170 - mesh 230 | 40 |
| 10 | …………………….. | API 200 - mesh 270 | 30 |
| 11 | …………………….. | API 230 - mesh 325 | 40 |

**Note**: Estimated values of Screens indicated in Appendix No. 1 are based on previous years usage, they are not binding and can be changed. The Buyer reserves the right to not purchase whole contracted volume or to purchase the Screens in amount that exceeds this volume after signing the Agreement.

1. **Documents requirements (at this and following pages please):**
2. enclose technical description of offered Screens that will cover with Exalo Drilling S.A. requirements,
3. enclose technical drawings of offered Screens that will cover with Exalo Drilling S.A. requirements,
4. enclose manufacturer’s quality documentation package,
5. enclose your API licenses related to Screens manufacturing.
6. **Terms of warranty**

Please enclose detailed description regarding to warranty terms for offered Screens in accordance with Appendix No. 1 – Technical Specification, point 5.

NOTE. Each page of enclosed documents must be numbered, dated, signed by authorized person and stamped.